;
; VAG-COM Redirect File 3W0-907-553.lbl
;
; VW Bentley Continental GT (3W)
;
; component: Level Control System (#34)
;
; p/n: 3D0 907 553 A
;      3D0 907 553 B Component: LUFTFDR.-CDC- 3C1V0 1101 (NAR and ROW Phaeton) - fully tested on this vehicle
;      3D0 907 553 C
;      3W0 907 553   Component: LUFTFDR.-CDC- 3C1V0 7014 (NAR and ROW Bentley) - not tested on this vehicle
;
; NOTE: both NAR and ROW Bentley Continental GT are coded 15500 by default.
;
; This file is part of a redirection package,
; make sure you have both of the following files.
;
; 3W0-907-553.lbl (this file)
; 3D0-907-553.lbl (the Phaeton ABS file that this redirect sends you to)
;
; by Michael Moore
; Moore@ross-tech.com
;
; created: 23/September/2005
;
; requires VAG-COM 405.0 or newer
;
;
REDIRECT,3W0-907-553.lbl,3W0-907-553-???
;
;
;Explanation of why this redirect file exists
;
;This file provides labels for the level control system on the Bentley Continental GT
;by calling up an existing label file for level control on the Phaeton.  It appears to 
;the author that both of these controllers (Phaeton and Bentley Continental GT) are identical, however, this
;label file has not been fully tested on the Bentley.
;
;