;
; VAG-COM Labelfile
;
; VW Touareg (7LA)
;
; Component: J104 - Brake Electronics (#03)
;
; P/N: 7L0-907-379-???
;
; includes coding and measuring groups
;
; created on 14/Oct/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 14/Oct/2005
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Brake Electronics (J104) Coding
C01,Model:
C02,+0000001 - Touareg (Through Part Number Index D)
C03,+0000002 - Touareg (From Part Number Index E)
C04, 
C05,Brakes:
C06,+0000000 - 16" Front Disc Brake (PR-1LB)
C07,+0008192 - 17" Front Disc Brake (PR-1LC/LD)
C08,+0016384 - 18" Front Disc Brake (PR-1LF)
C09, 
C10,Suspension:
C11,+0000000 - Standard Springs/Shocks (PR-1BA/BE)
C12,+0000128 - 4-Corner Air Suspension (PR-1BS/2BK)
C13,+0000256 - 4-Corner Air Suspension with electr. regluated Shocks (PR-1BK)
C14, 
C15,Transmission:
C16,+0006144 - Automatic & Manual Transmission (Through Part Number Index C)
C17, 
C18,+0004096 - Manual Transmission (From Part Number Index D)
C19,+0006144 - Automatic Transmission (From Part Number Index D)
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Current Wheel Speed
001,1,Speed Sensor,Front Left (G47),Specification: 0.0...255.0 km/h
001,2,Speed Sensor,Front Right (G45),Specification: 0.0...255.0 km/h
001,3,Speed Sensor,Rear Left (G46),Specification: 0.0...255.0 km/h
001,4,Speed Sensor,Rear Right (G44),Specification: 0.0...255.0 km/h
;
002,0,Starting Wheel Speed
002,1,Speed Sensor,Front Left (G47),Specification: 0.0...254.0 km/h (255.0 km/h = standing)
002,2,Speed Sensor,Front Right (G45),Specification: 0.0...254.0 km/h (255.0 km/h = standing)
002,3,Speed Sensor,Rear Left (G46),Specification: 0.0...254.0 km/h (255.0 km/h = standing)
002,4,Speed Sensor,Rear Right (G44),Specification: 0.0...254.0 km/h (255.0 km/h = standing)
;
003,0,Switches and Warning Lights
003,1,Brake Light,Switch (F),Specification: Not Oper./Operated
003,2,Brake System,Warning L. (K118),Specification: ON/OFF
003,3,ABS,Warning L. (K47),Specification: ON/OFF
003,4,ASR/ESP,Warning L. (K155),Specification: ON/OFF
;
004,0,Steering Angle / Lateral Acceleration / Rotation Rate
004,1,Steering Angle,,Specification: ± x.x °
004,2,Lateral,Acceleration,Specification: ± 1.5 m/s²
004,3,Rotation Rate,,Specification: ± 2.5 °/s
;
005,0,Brake Pressure
005,1,Brake Pressure,Sensor,Specification: ± 7.0 bar
;
006,0,Longitudinal Acceleration
006,1,Longitudinal,Acc. Sensor,Specification: ± 1.5 m/s²
;
007,0,Brake Pedal Path
007,1,Pedal Path,(Not Corrected)
007,2,Pedal Path,(Corrected)
007,3,Pedal Path,(Offset)
;
011,0,Speed Encoder Errors (Front Left)
;
012,0,Speed Encoder Errors (Front Right)
;
013,0,Speed Encoder Errors (Rear Left)
;
014,0,Speed Encoder Errors (Rear Right)
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine Electronics,,Specification: Engine 1\nDisplay Range: Engine 1/Engine 0
125,2,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nDisplay Range: Steer. ang. 1/Steer. ang. 0
125,3,All-Wheel-Drive,,Specification: AWD 1\nDisplay Range: AWD 1/AWD 0
125,4,Transmission,,Specification: Transm. 1\nDisplay Range: Transm. 1/Transm. 0
;
126,0,CAN-Databus Powertrain (Communication)
126,1,Instrument Cluster,,Specification: Instruments 1\nDisplay Range: Instruments 1/Instruments 0
126,2,CAN-Gateway,,Specification: Gateway 1\nDisplay Range: Gateway 1/Gateway 0
126,3,Level Control,,Specification: Level 1\nDisplay Range: Level 1/Level 0
;
127,0,CAN-Databus Powertrain (Communication)
127,1,Damper Control,,Specification: Damper Ctrl 1\nDisplay Range: Damper Ctrl 1/Damper Ctrl 0
127,2,Lock Electronics,,Specification: Lock-El. 1\nDisplay Range: Lock-El. 1/Lock-El. 0
;
