;
; VAG-COM labelfile
;
; component: R - Radio (#56) - ALPHA/BETA
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1C-56.LBL
; 1J-56.LBL
; 1J0-035-15x.LBL
; 1J0-035-18x.LBL
;
; created on 02/Jun/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 02/Jun/2005
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,GALA-Signal
001,2,Supply Voltage,(Terminal 30)
001,3,Illumination,(Terminal 58d)
001,4,Status,S-Contact
;
002,0,Speakers
002,1,Speakers,front
002,2,Status,,Specification: OK/short/open
;
003,0,Antenna
003,1,Antenna Type,,Specification: active/passive
003,2,Antenna
003,3,Status,,Specification: OK/short/open
;
004,0,Amplifier / Telephone-Mute
004,3,Telephone,Mute
004,4,Status,,Specification: on/off
;
005,0,CD-Player/Changer
005,1,CD-Drive
005,2,Status,,Specification: OK/n.OK
;
006,0,External Display
006,1,External Display
006,2,Status,,Specification: OK/n.OK
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C0,Radio (R) Coding
C1,0000?: Radio-Configuration
C2,+0 - Radio with passiver Antenna
C3,+1 - Active/Remote Supplied Antenna
C4,+2 - CD-Player/Changer
C5,+4 - External Display in Instrument Cluster
;
