;
; VAG-COM Labelfile
;
; VW Passat (3C)
;
; Component: J446 - Parking Aid (#76)
;
; P/N: 3C0-919-283-???
;
; includes measuring blocks, coding and adaptation
;
; created on 17/Dec/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 17/Dec/2005
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Distance (Rear)
001,1,Rear Left (G203),Sensor,Specification: 10...60 cm (255 cm = no obstacle recognized)
001,2,Rear Left (G204),Center Sensor,Specification: 10...160 cm (255 cm = no obstacle recognized)
001,3,Rear Right (G205),Center Sensor,Specification: 10...160 cm (255 cm = no obstacle recognized)
001,4,Rear Right (G206),Sensor,Specification: 10...60 cm (255 cm = no obstacle recognized)
;
002,0,Distance (Front)
002,1,Front Left (G255),Sensor,Specification: 10...60 cm (255 cm = no obstacle recognized)
002,2,Front Left (G254),Center Sensor,Specification: 10...120 cm (255 cm = no obstacle recognized)
002,3,Front Right (G253),Center Sensor,Specification: 10...120 cm (255 cm = no obstacle recognized)
002,4,Front Right (G252),Sensor,Specification: 10...60 cm (255 cm = no obstacle recognized)
;
003,0,Resulting Distance / Vehicle Speed && Voltage
003,1,Resulting,Distance Front,Specification: 10...120 cm (255 cm = no obstacle recognized)
003,2,Resulting,Distance Rear,Specification: 10...160 cm (255 cm = no obstacle recognized)
003,3,Vehicle Speed,,Display Range: 0.0...255.0 km/h
003,4,Sensor,Voltage Supply,Specification: 10.0...14.5 V
;
004,0,External Information
004,1,Reverese Gear,engaged,Display Range: Reverse: Yes/Reverse: No
004,2,Trailer hitched,,Display Range: YES/NO/Not Installed
004,3,Sound Output,Suppressed (Park),Display Range: OFF/ON
004,4,Parking Aid,Button (E266),Display Range: ON/OFF/Not Oper./Not Installed
;
005,0,Volume && Frequency
005,1,Rear Buzzer,Volume,Display Range: 1...9
005,2,Rear Buzzer,Frequency,Display Range: 1...9
005,3,Front Buzzer,Volume,Display Range: 1...9
005,4,Front Buzzer,Frequency,Display Range: 1...9
;
006,0,Oscillation Time (Rear)
006,1,Rear Left,Sensor,Specification: 0.8...1.5 ms
006,2,Rear Left,Center Sensor,Specification: 0.8...1.5 ms
006,3,Rear Right,Center Sensor,Specification: 0.8...1.5 ms
006,4,Rear Right,Sensor,Specification: 0.8...1.5 ms
;
007,0,Oscillation Time (Front)
007,1,Front Left,Sensor,Specification: 0.8...1.5 ms
007,2,Front Left,Center Sensor,Specification: 0.8...1.5 ms
007,3,Front Right,Center Sensor,Specification: 0.8...1.5 ms
007,4,Front Right,Sensor,Specification: 0.8...1.5 ms
;
008,0,Confirmation Sound
008,1,Confirm. Sound,(Reverse Gear),Display Range: ON/OFF
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A001,0,Rear Buzzer Volume
A001,1,Current Value
A001,5,Rear Buzzer Volume
A001,6,Adaptation of the rear warning buzzer volume.
A001,7, 
A001,8,Display Range: 1...9
;
A002,0,Rear Buzzer Frequency
A002,1,Current Value
A002,5,Rear Buzzer Frequency
A002,6,Adaptation of the rear warning buzzer frequency.
A002,7, 
A002,8,Display Range: 1...9
;
A003,0,Front Buzzer Volume
A003,1,Current Value
A003,5,Front Buzzer Volume
A003,6,Adaptation of the front warning buzzer volume.
A003,7, 
A003,8,Display Range: 1...9
;
A004,0,Front Buzzer Frequency
A004,1,Current Value
A004,5,Front Buzzer Frequency
A004,6,Adaptation of the front warning buzzer frequency.
A004,7, 
A004,8,Display Range: 1...9
;
A005,0,Confirmation Sound
A005,2,Current Status
A005,5,Confirmation Sound
A005,6,Adaptation of confirmation sound when
A005,7,switching into reverse gear.
A005,8, 
A005,9,135 = with confirmation sound
A005,10,136 = without confirmation sound
;
A006,0,Reset Factory Default
A006,5,Reset Factory Default
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Parking Aid (J446) Coding
C01,0?xxxxx: Suspension
C02,0 - Steel Suspension
C03,0x?xxxx: Trailer Hitch
C04,0 - without Trailer Hitch
C05,1 - with Trailer Hitch
C06,0xx?xxx: Transmission
C07,0 - Manual Transmission
C08,1 - Automatic Transmission
C09,0xxx?xx: Country
C10,0 - Rest of World (RoW)
C11,1 - USA/Canada/Japan
C12,0xxxx?x: Variant
C13,1 - Limousine (Sedan)
C14,2 - Variant (Wagon)
C15,0xxxxx?: Model
C16,4 - VW Passat (3C)
;
