;
; VAG-COM label file 6N0-909-901.lbl
;
; 19 - CAN Gateway
;
; Part #  6N0 909 901
;
; submitted by Davin Swanson
; modified by Sebastian Stange (sebastian@ross-tech.com) 14th March 2004
; modified by Michael Moore (moore@ross-tech.com) 30 August 2005 for Phaeton.
;
; NOTE: This controller is used in many cars, but the measuring blocks
;       are not present in every car. Also coding is different for each
;       controller/car. Part number is allways the same, without any indexes.
;
; ready for VAG-COM 500.9 and above
;
;---------------------------------------------------
;
; measured value block information
;
;---------------------------------------------------
;
;
001,0,*The first 9 blocks do not show error messages, but they do not show data either. 
;
002,0,*The first block known to have data in it is block 80
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,*This block not available. Next Available block is 125.
;
125,0,CAN-BUS Status (1 = OK / 0 = not OK)
125,1,Engine
125,2,Automatic, Transmission
125,3,ABS,Brake System
125,4,
;
126,0,CAN-BUS Status (1 = OK / 0 = not OK)
126,1,Steering, Angle
126,2,Airbag
126,3,
126,4,
;
127,0,CAN-BUS Status (1 = OK / 0 = not OK)
127,1,
127,2,AWD,
127,3,
127,4,
;
128,0,CAN-BUS Status (1 = OK / 0 = not OK)
128,1,Battery,Management
128,2,Electrical,Ignition Lock 1
128,3,Level control
;
129,0,Undocumented
;
130,0,CAN-BUS Status (1 = OK / 0 = not OK)
130,1,Comfort Can Bus,Mode,
130,2,Central,Convenience
130,3,Driver,Door
130,4,Passenger,Door
;
131,0,CAN-BUS Status (1 = OK / 0 = not OK)
131,1,Rear Right,Door
131,2,Rear Left,Door
131,3,Driver Seat,Memory
131,4,Electrical,Load Control
;
132,0,CAN-BUS Status (1 = OK / 0 = not OK)
132,1,
132,2,Steering,Wheel Electronics
132,3,Air Conditioning
132,4,Tire Pressure,Monitoring
;
133,0,CAN-BUS Status (1 = OK / 0 = not OK)
133,1,Roof,Electronics
133,2,Pax Seat,Memory
133,3,Rear Seat,Memory
133,4,Park Distance,Control
;
134,0,CAN-BUS Status (1 = OK / 0 = not OK)
134,1,
134,2,Electrical,Ignition Lock 1
134,3,Wiper Control,Module
134,4,
;
135,0,CAN-BUS Status (1 = OK / 0 = not OK)
135,1,
135,2,Display Control,Front 1
135,3,Display Control,Rear 1
134,4,
;
136,0,
136,1,
136,2,Central,Locking
136,3,
136,4,
;
137,0,*This block not available. Next Available block is 140.
;
138,0,*This block not available. Next Available block is 140.
;
139,0,*This block not available. Next Available block is 140.
;
140,0,Optical Data Bus Status (1 = OK / 0 = not OK)
140,1,Optical Data Bus,Mode,
140,2,
140,3,Navigation,System
140,4,
;
141,0,CAN-BUS Status (1 = OK / 0 = not OK)
141,1,
141,2,
141,3,
141,4,Telematics
;
142,0,CAN-BUS Status (1 = OK / 0 = not OK)
142,1,Display Control,Front 1
142,2
142,3,
142,4,
;
143,0,CAN-BUS Status (1 = OK / 0 = not OK)
143,1,Digital Sound,Processor,
143,2,
143,3,
143,4,
;
144,0,*This block not available. No further blocks available between here and 254.





