;
; VAG-COM label file
;
; VW Touareg (7L)
;
; component: level control system -J197- (#34)
;
; ECU p/n: 7L6 907 533 B/F
;
; includes measuring blocks, coding and adaption
;
; by Sebastian Stange
; sebastian@ross-tech.com
;
; last modified: 03/15/2004
;
; ready for VAG-COM 402.3 and above
;
;
;---------------------------------------------------
;
; Measuaring block informations
;
;---------------------------------------------------
;
;
001,0,Voltage and Speed
001,1,Voltage (Term.15),Specified Value: 0...20 V
001,2,Voltage (Term.30),Specified Value: 0...20 V
001,3,Speed
001,4,Terminal 50,(Starter),Specified Value: Term. 50 on/Term. 50 off
;
002,0,Door Status
002,1,Door Status
002,2,Tailgate Status
002,3,Power Supply,(right),Specified Value: 0...10 V
002,4,Power Supply,(left),Specified Value: 0...10 V
;
003,0,Switch and compressor status
003,1,Level control,switch selected
003,2,Dumper control, switch selected
003,3,[N/A]
003,4,Compressor,relay status
;
004,0,Level deviation from nominal level
004,1,Level deviation,front/left
004,2,Level deviation,front/right
004,3,Level deviation,rear/left
004,4,Level deviation,rear/right
;
005,0,Car heights in mm
005,1,Absolute height,front/left
005,2,Absolute height,front/right
005,3,Absolute height,rear/left
005,4,Absolute height,rear/right
;
006,0,Pressure and pressure accumulator
006,1,Compressor,temperature
006,2,Compressor,signal
06,3,Drain valve,status
006,4,Pressure,accumulator valve
;
007,0,Dump valves
007,1,Dump valve,front/left
007,2,Dump valve,front/right
007,3,Dump valve,rear/left
007,4,Dump valve,rear/right
;
008,0,Pitch angle
008,1,Pitch angle,increments
008,2,Pitch angle,duty cycle (%)
008,3,[N/A]
008,4,System Status
;
009,0,Long. Acceleration and Deviation
009,1,System Status
009,2,Longitudinal,Acceleration
009,3,Deviation,(front),Deviation from normal level.
009,4,Deviation,(rear),Deviation from normal level.
;
010,0,Level deviation from desired level.
010,1,Level deviation,front/left
010,2,Level deviation,front/right
010,3,Level deviation,rear/left
010,4,Level deviation,rear/right
;
011,0,Damper current
011,1,Damper current,front/left
011,2,Damper current,front/right
011,3,Damper current,rear/left
011,4,Damper current,rear/right
;
012,0,Buildup,acceleration
012,1,Buildup,acceleration (F/L)
012,2,Buildup,acceleration (F/R)
012,3,Buildup,acceleration (rear)
012,4,[N/A]
;
013,0,Damper speed
013,1,Damper speed,front/left,Neutral level: 2.5V
013,2,Damper speed,front/right,Neutral level: 2.5V
013,3,Damper speed,rear/left,Neutral level: 5V
013,4,Damper speed,rear/right,Neutral level: 5V
;
014,0,Damper and duty cycle status
014,1,Duty cycle,status
014,2,Damper status
014,3,[N/A]
014,4,[N/A]
;
015,0,Driving Information
015,1,Steering Angle
015,2,Speed
015,3,weighted,brake signal
015,4,CDC,limp mode
;
017,1,Regulation,requirement,Specified value: 0/1
;
023,3,Pressure,reservoir,Specified value: 1 = installed / 0 = not installed
;
080,0,Manufacturer work number and identification
; Date of manufacture
; Manufacturer changing status
; Manufacturer test stand no.
; Running manufacturer no.
; e.g. BPA = Bosch factory Ansbach
;
081,0,Vehicle Identification Number (VIN)
; Serial number
; Type test numbers
;
;
;---------------------------------------------------
;
; Coding informations
;
;---------------------------------------------------
;
;
C00,Touareg J197 Level Control Coding
C01,?xxxx - automatic vertical headlight (1 = not installed / 2 = installed)
C02,x?xxx - measurement of front axle
C03,(0 = -25mm / 1 = -20mm / 2 = -15mm / 3 = -10mm / 4 = -5mm)
C04,(5 = 0mm / 6 = +5mm / 7 = +10mm / 8 = +15mm / 9 = +20mm)
C05,xx?xx - measurement of rear axle
C06,(0 = -25mm / 1 = -20mm / 2 = -15mm / 3 = -10mm / 4 = -5mm)
C07,(5 = 0mm / 6 = +5mm / 7 = +10mm / 8 = +15mm / 9 = +20mm)
C08,xxx?x - vehicle type (2 = VW-E1-MAC)
C09,xxxx? - Country (0 = Rest of World / 1 = USA)
;
;
;---------------------------------------------------
;
; Adaptation informations
;
; this could rise/lower the air suspension
; login with security access code (function 16) before
; the correct login code will be 31564
;
;
;---------------------------------------------------
;
;
s