;
; VAG-COM label file
;
; VW Bora/Golf/Jetta (1J/9M) / VW New Bettle (1C/1Y/9C) / VW Sharan (7M)
;
; component: J567 - Automatic Headlight Aim Control Left (#29)
;
; p/n: 7M3-907-391
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 7M-29.LBL
; 7M-39.LBL
; 7M0-907-391-29.LBL
; 7M0-907-391-39.LBL
;
; created on 24/Aug/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 24/Aug/2005
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Basic Information (Basic Setting: Adjustment Position)
001,1,Voltage,Terminal 15
001,2,Voltage,Terminal 56b
001,3,Vehicle Speed
001,4,Vehicle Status,,0 = Vehicle is stationary\n85 = Vehicle moving uniformly\n255 = Vehicle not moving uniformly
;
002,0,Basic Information (Basic Setting: Position learning)
002,1,Front Level,Sender (G78),Specification: 1.6...3.0 V
002,2,Rear Level,Sender (G76),Specification: 2.0...3.0 V
002,3,Basic Setting,Status
002,4,Supply Voltage,Actuation Motor,Specification: 40...80 %
;
003,0,Basic Information
003,1,Bulb Output,,Specification: 30...40 W
003,2,Bulb Voltage,,Specification: 68...103 V
003,3,Supply Voltage,Act. Motor (Slave),Specification: 40...80 %
;
080,0,Advanced Control Module Identification I
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C0,Automatic Headlight Aim Control (J567) Coding
C1,00001 - Golf (FWD)
C2,00002 - Golf 4Motion (AWD)
C3,00003 - Bora (FWD)
C4,00004 - Bora 4Motion (AWD)
C5,00005 - Sharan
C6,00006 - New Beetle
;
