;
; VAG-COM Labelfile
;
; VW Golf/Jetta (1J/9M)
;
; component: J234 - Airbag (#15) - VW5/VW51/VW61
;
; P/N: 6Q0-909-605-??? / 1C0-909-60?-???
;
; includes measuring blocks and adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 6Q-15.LBL
; 6Q0-909-605-VW5.LBL  (VW5/VW51/VW61)
; 6Q0-909-605-VW52.LBL (VW52)
;
; created by Steve Tomasic (steve_tomasic@hotmail.com)
; updated on 09/Oct/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 09/Dec/2005
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
001,0,Ignitiers I (Front Airbags Stage 1 && Front Belt Tensioners)
001,1,Airbag (Stage 1),Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Airbag (Stage 1),Passenger Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Belt Tensioner,Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Belt Tensioner,Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
002,0,Ignitiers II (Rear Belt Tensioners)
002,1,Belt Tensioner,Rear Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Belt Tensioner,Rear Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,0,Voltage && Seat. Occupation && Belt Inquiry I (Front)
003,1,Voltage Supply,,Specification: Correct
003,2,Occupied Seat,Sensor Pass. Side,Display Range: child/child seat/light adult/heavy adult/occupied/not occupied/not installed
003,3,Belt Inquiry,Front Driver Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Front Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
004,0,Belt Inquiry II (Rear)
004,1,Belt Inquiry,Rear Driver Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
005,0,Igniters III (Side Airbags)
005,1,Side Airbag,Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,2,Side Airbag,Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,3,Side Airbag,Rear Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,4,Side Airbag,Rear Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
006,0,Seat Occupation (Rear)
006,1,Seat Occupation,Rear Driver Side,Display Range: Not Installed
006,2,Seat Occupation,Rear Pass. Side,Display Range: Not Installed
;
007,0,Igniters IV (Head Airbags)
007,1,Head-Level Airbag,Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
007,2,Head-Level Airbag,Passenger Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
008,0,Crash Sensor I (Version)
008,1,Driver Side,Front
008,2,Passenger Side,Front
008,3,Driver Side,Rear
008,4,Passenger Side,Rear
;
009,0,Crash Sensor I (Identification)
009,1,Driver Side,Front
009,2,Passenger Side,Front
009,3,Driver Side,Rear
009,4,Passenger Side,Rear
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A001,0,Front Passenger Airbag Deactivation
A001,1,Front Passenger,Airbag
A001,2,Current Status
A001,5,Front Passenger Airbag Deactivation
A001,6,0 - Airbag Enabled
A001,7,1 - Airbag Disabled
A001,8, 
A001,9,Note: Refer to Service Manual!
;
A002,0,Front Driver Airbag Deactivation
A002,1,Front Driver,Airbag
A002,2,Current Status
A002,5,Front Driver Airbag Deactivation
A002,6,0 - Airbag Enabled
A002,7,1 - Airbag Disabled
A002,8, 
A002,9,Note: Refer to Service Manual!
;
A003,0,Front Passenger Side Airbag Deactivation
A003,1,Front Passenger,Side Airbag
A003,2,Current Status
A003,5,Front Passenger Side Airbag Deactivation
A003,6,0 - Airbag Enabled
A003,7,1 - Airbag Disabled
A003,8, 
A003,9,Note: Refer to Service Manual!
;
A004,0,Front Driver Side Airbag Deactivation
A004,1,Front Driver,Side Airbag
A004,2,Current Status
A004,5,Front Driver Side Airbag Deactivation
A004,6,0 - Airbag Enabled
A004,7,1 - Airbag Disabled
A004,8, 
A004,9,Note: Refer to Service Manual!
;
A005,0,Front Passenger Belt Tensioner Deactivation
A005,1,Front Passenger,Belt Tensioner
A005,2,Current Status
A005,5,Front Passenger Belt Tensioner Deactivation
A005,6,0 - Belt Tensioner Enabled
A005,7,1 - Belt Tensioner Disabled
A005,8, 
A005,9,Note: Refer to Service Manual!
;
A006,0,Front Driver Belt Tensioner Deactivation
A006,1,Front Driver,Belt Tensioner
A006,2,Current Status
A006,5,Front Driver Belt Tensioner Deactivation
A006,6,0 - Belt Tensioner Enabled
A006,7,1 - Belt Tensioner Disabled
A006,8, 
A006,9,Note: Refer to Service Manual!
;
A007,0,Front Passenger Head Airbag Deactivation
A007,1,Front Passenger,Head Airbag
A007,2,Current Status
A007,5,Front Passenger Head Airbag Deactivation
A007,6,0 - Airbag Enabled
A007,7,1 - Airbag Disabled
A007,8, 
A007,9,Note: Refer to Service Manual!
;
A008,0,Front Driver Head Airbag Deactivation
A008,1,Front Driver,Head Airbag
A008,2,Current Status
A008,5,Front Driver Head Airbag Deactivation
A008,6,0 - Airbag Enabled
A008,7,1 - Airbag Disabled
A008,8, 
A008,9,Note: Refer to Service Manual!
;
