; For Audi A8 (4E), no guaranties
Byte 00 Bit 0 [69]	Trailer installed
Byte 00 Bit 1 [13]	Auto Distance regulation installed
Byte 00 Bit 2 [15]	Airbag system installed
Byte 00 Bit 3 [61]	Battery regulation installed
Byte 00 Bit 4 [38]	Roof electronic installed
Byte 00 Bit 5 [03]	Anti-lock brake (ABS) installed
Byte 00 Bit 6 [53]	Parking Brake installed
Byte 00 Bit 7 [76]	Park Assist installed
Byte 01 Bit 0 [1D]	Driver identification installed
Byte 01 Bit 1 [05]	Zugangs- und Startberechtigung installed
Byte 01 Bit 2 [25]	Immobilizer installed
Byte 01 Bit 3 [19]	CAN-Gateway installed (Standard)
Byte 01 Bit 4 [02]	Automatic transmission installed
Byte 01 Bit 5 [09]	Central Electronics installed
Byte 01 Bit 6 [4F]	Central Electronics II installed
Byte 01 Bit 7 [46]	Central Convenience installed
Byte 02 Bit 0 [17]	Instrument Cluster installed
Byte 02 Bit 1 [08]	Auto HVAC installed
Byte 02 Bit 2 [28]	Auto HVAC rear installed
Byte 02 Bit 3 [34]	Level control installed
Byte 02 Bit 4 	Steering Wheel Sensor installed (G85)
Byte 02 Bit 5 [55]	Xenon Range installed
Byte 02 Bit 6 [01]	Engine I installed
Byte 02 Bit 7 [11]	Engine II installed
Byte 03 Bit 0 [65]	Tire Pressure Monitoring installed
Byte 03 Bit 1 [18]	Auxiliary Heating installed
Byte 03 Bit 2 [16]	Steering Wheel electronic installed
Byte 03 Bit 3 [36]	Seat Memory (Driver) installed
Byte 03 Bit 4 [06]	Seat Memory (Passenger) installed
Byte 03 Bit 5 [66]	Seat Memory (Rear) installed
Byte 03 Bit 6 [42]	Door Electronics (Driver) installed
Byte 03 Bit 7 [52]	Door Electronics (Passenger) installed
Byte 04 Bit 0 [62]	Door Electronics (Rear Left) installed
Byte 04 Bit 1 [72]	Door Electronics (Rear Right) installed
Byte 04 Bit 2 [27]	Control Head (Rear) installed
Byte 04 Bit 3 [07]	Control Head installed
Byte 04 Bit 4 [0E]	Mediaplayer Position 1 installed
Byte 04 Bit 5 [1E]	Mediaplayer Position 2 installed
Byte 04 Bit 6 [2E]	Mediaplayer Position 3 installed
Byte 04 Bit 7 [3E]	Mediaplayer Position 4 installed
Byte 05 Bit 0 [56]	Radio (Analog) installed
Byte 05 Bit 1 [75]	Telematic/Emergency Call installed
Byte 05 Bit 2 [57]	TV-Tuner installed
Byte 05 Bit 3 [0F]	Radio (Digital) installed
Byte 05 Bit 4 [77]	Phone installed
Byte 05 Bit 5 [37]	Navigation system installed
Byte 05 Bit 6 [67]	Voice Control installed
Byte 05 Bit 7 [4E]	Control Head (Rear right) installed
Byte 06 Bit 0 [5E]	Control Head (Rear left) installed
Byte 06 Bit 1 [1F]	Radio (Satellit) installed
Byte 06 Bit 2 [47]	Sound System installed
Byte 06 Bit 3 
Byte 06 Bit 4 
Byte 06 Bit 5 
Byte 06 Bit 6 
Byte 06 Bit 7 
