;
; VAG-COM Measuring Block Labels for
; US OBD-II VR6, ECU p/n 021-906-259-xx
;
1,0,General Engine Data
1,1,,Engine Speed
1,2,Coolant,Temperature
1,3,Oxygen Sensor,Regulation
1,4,Ignition,Timing
;
2,0,General Engine Data
2,1,,Eng Speed
2,2,Injector,ON Time
2,3,Battery,Voltage
2,4,,[unknown]
;
3,0,Engine Load Registration 1
3,1,,Engine Speed
3,2,Mass Air Flow,
3,3,Throttle Angle,
3,4,Intake Air,Temperature
;
5,0,General Engine Data
5,1,,Engine Speed
5,2,Engine Load, 
5,3,Vehicle,Speed
5,4,Operating,Mode
;
8,0,Signals to ECU
8,1,,Engine Speed
8,2,Drive Range,Status
8,3,A/C Status
8,4,A/C Comp.,Status
;
10,0,Ignition 1
10,1,,Engine Speed
10,2,Engine Load,
10,3,Ignition Timing,From Map
10,4,Ignition Timing,Actual
;
15,0,Engine Load Registration 1
15,1,,Engine Speed
15,2,Engine Load, 
15,3,Engine Load, 
15,4,Mass Air Flow, 
;
16,0,Engine Load Registration 2
16,1,,Engine Speed
16,2,,Engine Load,
16,3,,Engine Load,
16,4,Load Calc. from,Throttle Angle
;
25,0,Oxygen Sensor Before CAT (B1-S1)
25,1,Oxygen Sensor,Regulation
25,2,O2S Adaptation,Partial Load
25,3,O2S Adaptation,Idle
25,4,O2S Control,Status
;
36,0,Idle Control
36,1,Throttle,Angle
36,2,Mass Air Flow,Idle Adaptation
36,3,Mass Air Flow,Driving Adaptation
36,4,[Empty],
;
37,0,Idle Control
37,1,,Engine Speed
37,2,,Specification
37,3,Idle Control,
37,4,Mass Air Flow,
;
45,0,Knock Control (Cyl 1-4) 
45,1,Ign. Angle Cor., Cylinder 1
45,2,Ign. Angle Cor., Cylinder 2
45,3,Ign. Angle Cor., Cylinder 3
45,4,Ign. Angle Cor., Cylinder 4
;
46,0,Knock Control (Cyl 5-6) 
46,1,Ign. Angle Cor., Cylinder 5
46,2,Ign. Angle Cor., Cylinder 6
46,3,[empty]
46,4,[empty]
;
47,0,Knock Sensor [Undocumented]
47,1,,Cylinder 1
47,2,,Cylinder 2
47,3,,Cylinder 3
47,4,,Cylinder 4
;
48,0,Knock Sensor [Undocumented]
48,1,,Cylinder 5
48,2,,Cylinder 6
48,3,[empty]
48,4,[empty]
;
98,0,Throttle Control Basic Setting
98,1,Throttle Pot, Voltage 1
98,2,Throttle Pot, Voltage 2
98,3,Operating Mode,
98,4,Basic Setting,Status
;
103,0,[Undocumented]
103,1,,Engine Speed
103,2,,Coolant
103,3,CAT Temp,(Calculated)
103,4,,Status
;
110,0,Misfire Detection 1
110,1,Engine Load,
110,2,Misf. Count, Imp. Exh. Gas
110,3,Misf. Count, Impair Cat
110,4,Misf. Det.,Status
;
115,0,Oxygen Sensor Before CAT (B1-S1)
115,1,Coolant,Tempertaure
115,2,Exh. Gas Temp,(Calculated)
115,3,,Oxygen Sensor
115,4,,Control,Status
;
116,0,Oxygen Sensor Behind CAT (B1-S2)
116,1,Regulation,Time
116,2,Exh. Gas Temp,(Calculated)
116,3,,Oxygen Sensor
116,,Control Status
;
120,0,Oxygen Sensor Heating Before CAT (B1-S1) 
120,1,Exh. Gas Temp,(Calculated)
120,2,O2S Time to Start,After Heater ON
120,3,,O2S Resistance
120,4,,Control Status 
;
121,0,Oxygen Sensor Heating Behind CAT (B1-S2) 
121,1,CAT Temp,(Calculated)
121,2,Time to Start,After Heater ON
121,3,,Sensor Resistance
121,4,,Control Status 
;
125,0,[Undocumented]
125,1,,Engine Speed
125,2,Oxygen Sensor,Adaptation
125,3,Oxygen Sensor,Control
125,4,,Status
;
130,0,Oxygen Sensor Ageing Before CAT (B1-S1) 
130,1,,Engine Speed
130,2,Cycle Time,(Frequency)
130,3,Valid Cycles,Counted
130,4,,Control Status
;
131,0,Oxygen Sensor Ageing Behind CAT (B1-S2)
131,1,,Engine Speed
131,2,,Oxygen Sensor
132,3,Extended Signal,Frequency
131,4,,Control Status
;
136,0,[Undocumented]
136,1,,Engine Speed
136,2,CAT Temp,(calculated)
136,3,Cat Efficiency,
136,4,,Status
;
140,0,[Undocumented -- Throttle Control]
;
141,0,[Undocumented -- Throttle Control]
;
142,0,[Undocumented -- Throttle Control]
142,1,Throttle,Position
142,2,T.P.,Minumim
142,3,T.P.,Maximum
142,4,,Status
;
