;
; VAG-COM Labelfile
;
; VW Passat (3C)
;
; Component: J540 - Parking Brake (#53)
;
; P/N: 3C0-907-801-???
;
; includes measuring blocks, coding and adaptation
;
; created on 09/April/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification: 09/Nov/2005
;
; requires VAG-COM 402.3 or newer
;
;
;---------------------------------------------------
;
; measuring block information
;
;---------------------------------------------------
;
;
002,2,Parking Brake,Button (E538)
002,4,Auto Hold,Button (E540)
;
007,2,Rear left brake,operating counter
007,3,Rear right brake,operating counter
;
008,2,Clutch pedal,switch (F36) path,Display Range: 0...250 (250 = 100 %)
;
010,2,Parking brake,last operation,Displayed value has to be multiplied by 8 - the result is the KM reading of the last parking brake activation.
;
011,2,Parking Brake,Indicator Lamp,K213
011,3,Auto Hold,Indicator Lamp,K238
011,4,ABS (J104) Control,Module coding
;
012,1,AUTO HOLD,Status
012,2,Parking brake,Status
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Brake Electronics,,Specification: ABS 1\nDisplay Range: ABS 1/ABS 0
125,2,Airbag,,Specification: Airbag 1\nDisplay Range: Airbag 1/Airbag 0
125,3,Transmission,,Display Range: Transm. 1/Transm. 0
125,4,Engine,,Specification: Engine 1\nDisplay Range: Engine 1/Engine 0
;
126,0,CAN-Databus Powertrain (Communication)
126,1,CAN-Gateway,,Specification: Gateway 1\nDisplay Range: Gateway 1/Gateway 0
126,3,Ignition Lock,,Specification: El.Ign.Lock 1\nDisplay Range: El.Ign.Lock 1/El.Ign.Lock 0
;
225,0,CAN-Databus Powertrain (Time-Out)
225,1,Brake Electronics
225,2,Airbag
225,3,Transmission
225,4,Engine
;
226,0,CAN-Databus Powertrain (Time-Out)
226,1,CAN-Gateway
226,3,Ignition Lock
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A20,0,Rear Left Brake Adaptation
A20,5,Rear Left Brake Adaptation
A20,6,Save 0 to reset the adaptation.
;
A21,0,Rear Right Brake Adaptation
A21,5,Rear Right Brake Adaptation
A21,6,Save 0 to reset the adaptation.
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Parking Brake (J540) Coding
C01,0000011 - Parking Brake without Auto-Hold (Rest of World / PR-UH1)
C02,0000012 - Parking Brake with Auto-Hold (Rest of World / PR-UH2)
C03,0000013 - Parking Brake with Auto-Hold (USA) "UNDOCUMENTED"
;
;
;---------------------------------------------------
;
; selective output test information
;
;---------------------------------------------------
;
;
; 2442 - Electric Park/Handbrake Indicator Lamp (K213)
; 2573 - Rear Left Parking Brake Motor (V282)
; 2575 - Rear Right Parking Brake Motor (V283)
; 2576 - Open Rear Parking Brake Motors (V282 & V283)
; 2578 - Close Rear Parking Brake Motors (V282 & V283)
; 2844 - Auto Hold Indicator Lamp 1 (K237) and 2 (K238)
; 2845 - Brake System Warning Lamp (K118)
;
